| iTool User's Guide: Operations Properties |

## Map Register Image Properties

The map projection functionality displays image and contour data that are georeferenced and mapped to particular projections. See Working with Maps for details on how to use mapping functionality.

Map Register Image has the following configurable properties.

Table C-27: Map Register Properties

Table C-27: Map Register Properties
Property | Control Type: Options
--- | ---
Origin (x) | Number: Set the longitudinal minimum in degrees. Default = `0`
End (x) | Number: Set the longitudinal maximum in degrees. Default = `0`
Pixel size (x) | Number: Set the longitudinal pixel size in degrees. Default = `0`
Origin (y) | Number: Set the latitudinal minimum in degrees. Default = `0`
End (y) | Number: Set the latitudinal maximum in degrees. Default = `0`
Pixel size (y) | Number: Set the latitudinal pixel size in degrees. Default = `0`

IDL Online Help (March 01, 2006)